\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Application Instructions**

**TOOLS:**

* Sharp razor knife
* Ammonia based window cleaner or Acetone (Preferred)
* Tape

**VIDEOS OF INSTALLATION:**

* Watch a video of installation at: [www.aquamarinedeck.com](http://www.aquamarinedeck.com)

**STORAGE:**

* Should be stored flat in a cool, dry, indoor location until installed

**LIMITATIONS:**

* Do NOT install in temperatures below 60 degrees
* Do NOT attempt to remove and adjust placement once pad is down

**PREPARATION:**

* Clean surfaces followed by acetone on the area to be covered. Thoroughly clean all surface areas.
* Make sure all grease, adhesive, mold-release; wax and other substances are removed before installing the product. The area must be completely dry before applying Aqua Marine Deck product.
* All snaps must be removed and holes filled with JB Water Weld or caulk

**INSTALLATION: \*DO NOT PULL OR STRETCH THE PAD(S)\***

1. Before you peel back the adhesive backing, place the pads on the surface area to verify the fit and spacing in order to determine the exact location of the pad(s).
2. Turn pad over so that the adhesive backing is face up. With a sharp razor knife carefully cut the paper adhesive backing down the center. Cut through the adhesive, but DO NOT cut into the pad.
3. Peel back and fold the four corners of the paper backing.
4. Turn the pad back over and reposition it.
5. Secure one side of the pad to the surface area using tape. Taping prevents the pad from moving.
6. Lift up the side that is not taped down and pull up the folded corners.
7. From the center working towards the outer edges, slowly peel the rest of the paper backing while applying pressure to the pad to ensure there’s a firm bond to the surface area.
8. Remove the masking tape from the other side of the pad and repeat step 7.
9. Roll firmly, pressing down on all surface areas and especially the edges of the pad to ensure there’s a good adhesive. The 3M adhesive backing takes 14 PSI to activate. We recommend using the Kobalt Extension Handle Roller found at your local Lowe’s Home Improvement Store.

**MAINTENANCE:**

1. NEVER use a pressure washer or bleach to clean the material.
2. Clean decking with a soft carwash brush and Tide Liquid Laundry Soap
3. Aqua Marine Deck sells EVA foam cleaner for purchase. Call for details.